**MDX Platform technical information**

Festo:

IP Address: 192.168.0.10

Port: 991

protocol: propriatery (Festo easyIP)

NoLimits telemetry:

IP Address: 192.168.0.4 (the address of the VR PC)

Port: 15151

Protocol: propriatery (documented in NoLimits distribution)

Condor(flight sim:

IP Address: 192.168.0.4 (the address of the VR PC)

Port: 55278

Protocol: proprietary (documented in distribution)

Elite Dangerous:

IP Address: 192.168.0.4 (the address of the VR PC)

Port: 5150

Protocol: under development

Platform Runtime:

IP Address is either VR PC or Pi controller

V1 platform input port: 10002 (deprecated)

Generic IP Client port: 10009

NoLimits coaster client port : 10011

Orientation Display output port: 10020 (contains UDP orientation messages)

Monitor output port: 10010 (UDP orientation test messages)

Client remote controller messages: 10013